    COMMAND		OPERATION			SYNTAX		STATUS AFFECTED		TUTORIAL
    ADDLW     	ADD Literal to W             	ADDLW K    	C, DC, Z 		7
    ADDWF    	ADD W to F                  	ADDWF F,D  	C, DC, Z    	        7
    ANDLW     	AND Literal and W            	ANDLW K    	Z          		7
    ANDWF     	AND W with F                 	ANDWF F,D  	Z          		7
    BCF       	Bit Clear F                  	BCF   F,B  	None        	        2
    BSF      	Bit Set F                    	BSF   F,B  	None        	        2
    BTFSC    	Bit Test, Skip if Clear      	BTFSC F,B  	None       		4
    BTFSS     	Bit Test, Skip if Set        	BTFSC F,B  	None        	        4
    CALL      	Subroutine Call              	CALL K     	None        	       13
    CLRF      	Clear F                      	CLRF F     	Z          		2
    CLRW      	Clear W register             	CLRW      	Z           		2
    CLRWDT    	Clear Watchdog Timer         	CLRWDT     	TO, PD		       30
    COMF     	Complement F                 	COMF F,D   	Z           	       11
    DECF      	Decrement F                 	DECF F,D   	Z           		6
    DECFSZ   	Decrement F, Skip if 0       	DECFSZ F,D 	None        	        6
    GOTO      	Unconditional branch         	GOTO K    	None        	        3
    INCF      	Increment F                  	INCF F,D   	Z           		6
    INCFSZ   	Increment F, Skip if 0       	INCFSZ F,D 	None        	        6
    IORLW     	Inclusive OR Literal with W 	IORLW K    	Z           	       17
    IORWF     	Inclusive OR W with F        	IORWF F,D  	Z           	       17
    MOVF      	Move F                       	MOVF F,D   	Z           		5
    MOVLW     	Move Literal to W            	MOVLW K   	None        	        4
    MOVWF     	Move W to F                  	MOVWF F   	None        	        4
    NOP       	No Operation                 	NOP       	None         	       12
    RETFIE    	Return from Interrupt        	RETFIE    	None       	       28
    RETLW     	Return with Literal in W     	RETLW K   	None        	       13
    RETURN    	Return from Subroutine      	RETURN     	None        	       13
    RLF       	Rotate Left through Carry    	RLF F,D    	C           		4
    RRF      	Rotate Right through Carry   	RRF F,D    	C           		4
    SLEEP     	Power-down                  	SLEEP      	TO, PD      	       29
    SUBLW    	Subtract W from Literal      	SUBLW K    	C, DC, Z    	       23
    SUBLW     	Subtract W from F            	SUBWF F,D  	C, DC, Z    	       23
    SWAPF     	Swap F                       	SWAPF F,D  	None       	       11
    XORLW     	Exclusive OR Literal with W  	XORLW K    	Z           	       17
    XORWF    	Exclusive OR W with F       	XORWF F,D  	Z           	       17

    LEGENDS

    C	 Carry
    b	 Bit address
    C	 Carry
    d	 Destination
    DC	 Digit Carry
    f	 Register File Address
    k	 Literal or label
    PD	 Power-down
    TO	 Time-out
    W	 Working Register
    Z	 Zero