    REGISTER	ADDRESS	POWER-ON 	MCLR RESET	WAKE UP
    			RESET				FROM SLEEP
    W		-	xxxx xxxx	uuuu uuuu	uuuu uuuu
    INDF		00h	---- ---- 	---- ----	---- ----
    TMRO		01h	xxxx xxxx	uuuu uuuu	uuuu uuuu
    PCL		02h	000h		0000h		PC +1 (2)
    STATUS		03h	0001 1xxx	000? ?uuu(3)	uuu? ?uuu(3)
    FSR		04h	xxxx xxxx	uuuu uuuu	uuuu uuuu
    PORTA		05h	---u uuuu	---u uuuu	---u uuuu
    PORTB		06h	xxxx xxxx	uuuu uuuu 	uuuu uuuu
    EEDATA		08h	xxxx xxxx	uuuu uuuu 	uuuu uuuu
    EEADR		09h	xxxx xxxx	uuuu uuuu 	uuuu uuuu
    PCLATH		0Ah	---0 0000	---0 0000	---u uuuu
    INTCON		0Bh	0000 000x	0000 000u	0000 000(1)
    INDF		80h	---- ----	---- ----	---- ----
    OPTION		81h	1111 1111	1111 1111	uuuu uuuu
    PCL		82h	0000h		0000h		PC +1
    STATUS		83h	0001 1xxx	000? ?uuu(3)	uuu? ?uuu(3)
    FSR		84h	xxxx xxxx	uuuu uuuu	uuuu uuuu
    TRISA		85h	---1 1111	---1 1111	---u uuuu
    TRISB		86h	1111 1111	1111 1111	uuuu uuuu
    EECON1		88h	---0 0000	---0 ?000	---0 ?uuu
    EECON2		89h	---- ----	---- ----	---- ----
    PCLATH		8Ah	---0 0000	---0 0000	---u uuuu
    INTCON		8Bh	0000 000x	0000 000u	uuuu uuuu(1)

    Legend
      	u = unchanged
    	x = unknown
    	- = unimplemented bit read as '0'
    	? = value depends on condition

    Notes:
    (1) = One or more bits in INTCON will be affected (to cause wake-up)
    (2) = When the wake-up is due to an interrupt and the GIE bit is set,
          the PC is loaded with the interrupt vector (0004h)
    (3) = See PIC datasheet for reset values for each condition