PPPv3.1 Release Notes
=====================


v3.3.6.17
---------

Date: 10/03/2005

 * Added support for the following devices:
     - PIC18F2410, PIC18F2420, PIC18F2455, 
     - PIC18F2510, PIC18F2520, PIC18F2550
     - PIC18F4410, PIC18F4420, PIC18F4455, PIC18F4510
     - PIC18F6310, PIC18F6390, PIC18F6625, PIC18F6721
     - PIC18F8310, PIC18F8390, PIC18F8625, PIC18F8721

 * Support for firmware Vdd switching (>= v4) on new USB boards
     - including option to specify Vdd raise timing
     - also added LVP scripts for Vdd switching
     
 * Implemented "simple" mode configuration screen for popular chips
 
 * Warning when programming MCLR internal to avoid problems on older hardware
 
 * Removed "obj" file reference from open dialog
 
 * Added support for V3 Dev Board


v3.2.5.13
---------

 * Added support for the following devices:
     - PIC12F683
     - PIC12F635
     - PIC16F636
     
 * New "Erase with Vdd Msg" button in the debug screen to allow 
   chips with "internal MCLR / RB6" issue to be erased.
   
 
v3.1.4.12
---------

  * Major revision of PPP - it is now compatible with most PIC18F devices


