Run Program 1.1 and verify that the LED on the bottom bit (bit 0) of PORTA lights. Use the crystal clock (set the switch to RC). The LED should light the instant that you press the RESET button. Since the PICmicro is reset when it starts up you will find that the LED comes on the instant we turn the power on.

The LED should light the instant that you press the RESET button. Since the PICmicro is reset when it starts up you will find that the LED comes on the instant we turn the power on.