PROTO-SPHERA  EXPERIMENT- preliminary layout

The size and the feature of PROTO-SPHERA Experiment has required an investigation on Frascati Laboratory site to select a possible location

which would have provided an appropriate number of facilities.

The ex FT machine experimental hall was appearing to be a suitable location for the new experiment.

The protosphera experimental machine, as proposed in the layout drawings (no ELE-A-PS-001-L sheet 1 & 2), can be installed on top of a new platform, which can be erected off-centre at the hall entrance.

The height and the plan arrangement of this platform will allow:

· A good access underneath the machine for the various services

· A full extraction of the interior part of machine from its tank by the existing top crane.

· A free loading area from the main hall entrance.

· An accessible and adeguate area around the new machine for service routes and maintenance.

· A short distance from the available area of the basement where is possible to install most of the power supply equipment.

· A good contiguous room, at the experiment level, available for the installation of engineering and diagnostic control apparatus.

For the erection of the new platform it is necessary to reduce the length of the existing one (only for 2.5 m).  This, nevertheless, will not impair the

operation of the FT machine whenever required.
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